[general]
version = 1
name = Normal Quality
machine_type = ultimaker2plus
machine_variant = 0.4 mm
material = CPE

[settings]
retraction_hop = 0.0
support_enable = False
raft_airgap = 0.0
raft_surface_thickness = 0.27
support_pattern = lines
raft_interface_line_spacing = 3.0
skin_no_small_gaps_heuristic = False
raft_surface_line_width = 0.4
cool_fan_speed_min = 50
retraction_combing = All
adhesion_type = brim
cool_min_layer_time = 3
infill_before_walls = False
speed_layer_0 = 20
brim_line_count = 20
cool_lift_head = True
raft_interface_line_width = 0.4
cool_fan_speed_max = 100
magic_mesh_surface_mode = False
speed_print = 20
shell_thickness = 1.05
speed_wall_0 = 20
material_flow = 100.0
raft_surface_line_spacing = 3.0
raft_margin = 5.0
retraction_speed = 40.0
layer_height_0 = 0.26
material_bed_temperature = 70
speed_wall_x = 30
infill_overlap = 15
speed_infill = 45
skirt_minimal_length = 150.0
speed_topbottom = 20
skirt_gap = 3.0
raft_base_line_width = 1.0
machine_nozzle_size = 0.35

