[general]
version = 1
name = Normal Quality
machine_type = ultimaker2plus
machine_variant = 0.8 mm
material = ABS

[settings]
raft_surface_thickness = 0.27
raft_base_line_width = 1.0
raft_margin = 5.0
cool_min_layer_time = 3
support_enable = False
retraction_combing = All
cool_min_speed = 15
brim_line_count = 10
top_thickness = 1.2
material_flow = 100.0
cool_lift_head = True
speed_print = 20
retraction_hop = 0.0
machine_nozzle_size = 0.7
layer_height = 0.2
speed_wall_0 = 20
raft_interface_line_spacing = 3.0
speed_topbottom = 20
speed_infill = 40
infill_before_walls = False
retraction_speed = 40.0
skin_no_small_gaps_heuristic = False
shell_thickness = 2.1
cool_fan_speed_max = 100
raft_airgap = 0.0
material_bed_temperature = 70
infill_overlap = 15
speed_wall_x = 30
skirt_minimal_length = 150.0
speed_layer_0 = 20
bottom_thickness = 1.2
layer_height_0 = 0.5
magic_mesh_surface_mode = False
cool_fan_speed_min = 50
top_bottom_thickness = 1.2
skirt_gap = 3.0
raft_interface_line_width = 0.4
adhesion_type = brim
support_pattern = lines
raft_surface_line_width = 0.4
raft_surface_line_spacing = 3.0

