Smart Array P400i in Slot 0 (Embedded)
   Bus Interface: PCI
   Slot: 0
   Serial Number: REDACTED
   Cache Serial Number: REDACTED
   RAID 6 (ADG) Status: Enabled
   Controller Status: OK
   Hardware Revision: E
   Firmware Version: 7.24-0
   Rebuild Priority: Medium
   Expand Priority: Medium
   Surface Scan Delay: 15 secs
   Surface Scan Mode: Idle
   Parallel Surface Scan Supported: No
   Elevator Sort: Enabled
   Wait for Cache Room: Disabled
   Surface Analysis Inconsistency Notification: Disabled
   Post Prompt Timeout: 0 secs
   Cache Board Present: True
   Cache Status: Temporarily Disabled
   Cache Status Details: Cache disabled; low batteries.
   Cache Ratio: 25% Read / 75% Write
   Drive Write Cache: Disabled
   Total Cache Size: 256 MB
   Total Cache Memory Available: 208 MB
   No-Battery Write Cache: Disabled
   Cache Backup Power Source: Batteries
   Battery/Capacitor Count: 1
   Battery/Capacitor Status: Failed (Replace Batteries)
   SATA NCQ Supported: True
   Number of Ports: 2 Internal only
   Driver Name: cciss
   Driver Version: 3.6.26
   PCI Address (Domain:Bus:Device.Function): 0000:06:00.0
   Port Max Phy Rate Limiting Supported: False
   Host Serial Number: REDACTED
   Sanitize Erase Supported: False
   Primary Boot Volume: None
   Secondary Boot Volume: None


   Port Name: 1I
         Port ID: 0
         Port Connection Number: 0
         SAS Address: 0000000000000000
         Port Location: Internal

   Port Name: 2I
         Port ID: 1
         Port Connection Number: 1
         SAS Address: 0000000000000000
         Port Location: Internal


   Internal Drive Cage at Port 1I, Box 1, OK

      Power Supply Status: Not Redundant
      Drive Bays: 4
      Port: 1I
      Box: 1
      Location: Internal

   Physical Drives
      physicaldrive 1I:1:1 (port 1I:box 1:bay 1, SATA HDD, 250 GB, OK)
      physicaldrive 1I:1:2 (port 1I:box 1:bay 2, SATA HDD, 250 GB, OK)
      physicaldrive 1I:1:3 (port 1I:box 1:bay 3, SATA HDD, 100 GB, OK)
      physicaldrive 1I:1:4 (port 1I:box 1:bay 4, SATA HDD, 100 GB, OK)



   Internal Drive Cage at Port 2I, Box 1, OK

      Power Supply Status: Not Redundant
      Drive Bays: 2
      Port: 2I
      Box: 1
      Location: Internal

   Physical Drives
      None attached


   Array: A
      Interface Type: SATA
      Unused Space: 0  MB (0.0%)
      Used Space: 186.3 GB (100.0%)
      Status: OK
      Array Type: Data


      Logical Drive: 1
         Size: 93.1  GB
         Fault Tolerance: 1
         Heads: 255
         Sectors Per Track: 32
         Cylinders: 23934
         Strip Size: 128 KB
         Full Stripe Size: 128 KB
         Status: OK
         Caching:  Enabled
         Unique Identifier: 600508B1001038333220202020200004
         Disk Name: /dev/cciss/c0d0
         Mount Points: /boot 94 MB Partition Number 1, / 91.2 GB Partition Number 3
         OS Status: LOCKED
         Logical Drive Label: A00AD958PH89MQ7832     7E6D
         Mirror Group 1:
            physicaldrive 1I:1:3 (port 1I:box 1:bay 3, SATA HDD, 100 GB, OK)
         Mirror Group 2:
            physicaldrive 1I:1:4 (port 1I:box 1:bay 4, SATA HDD, 100 GB, OK)
         Drive Type: Data
         LD Acceleration Method: Controller Cache


      physicaldrive 1I:1:3
         Port: 1I
         Box: 1
         Bay: 3
         Status: OK
         Drive Type: Data Drive
         Interface Type: SATA
         Size: 100 GB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Firmware Revision: 6PB10362
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     INTEL SSDSA2BZ10
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 23
         Maximum Temperature (C): 32
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 1I:1:4
         Port: 1I
         Box: 1
         Bay: 4
         Status: OK
         Drive Type: Data Drive
         Interface Type: SATA
         Size: 100 GB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Firmware Revision: 6PB10362
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     INTEL SSDSA2BZ10
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 23
         Maximum Temperature (C): 33
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None


   Unassigned

      physicaldrive 1I:1:1
         Port: 1I
         Box: 1
         Bay: 1
         Status: OK
         Drive Type: Unassigned Drive
         Interface Type: SATA
         Size: 250 GB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Firmware Revision: 0001EXM1
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     ST250LT021-1AF14
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 28
         Maximum Temperature (C): 36
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 1I:1:2
         Port: 1I
         Box: 1
         Bay: 2
         Status: OK
         Drive Type: Unassigned Drive
         Interface Type: SATA
         Size: 250 GB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Firmware Revision: 0001EXM1
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     ST250LT021-1AF14
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 28
         Maximum Temperature (C): 36
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None
