Adapter #0

Number of Virtual Disks: 1
Virtual Drive: 0 (Target Id: 0)
Name                :Virtual Disk 0
RAID Level          : Primary-1, Secondary-0, RAID Level Qualifier-0
Size                : 3.491 TB
Sector Size         : 512
Is VD emulated      : No
Mirror Data         : 3.491 TB
State               : Optimal
Strip Size          : 64 KB
Number Of Drives    : 8
Span Depth          : 1
Default Cache Policy: WriteBack, ReadAhead, Direct, No Write Cache if Bad BBU
Current Cache Policy: WriteBack, ReadAhead, Direct, No Write Cache if Bad BBU
Default Access Policy: Read/Write
Current Access Policy: Read/Write
Disk Cache Policy   : Disk's Default
Encryption Type     : None
Default Power Savings Policy: Controller Defined
Current Power Savings Policy: None
Can spin up in 1 minute: No
LD has drives that support T10 power conditions: No
LD's IO profile supports MAX power savings with cached writes: No
Bad Blocks Exist: No
PI type: No PI

Is VD Cached: No
Number of Spans: 1
Span: 0 - Number of PDs: 8

PD: 0 Information
Enclosure Device ID: 32
Slot Number: 0
Drive's position: DiskGroup: 0, Span: 0, Arm: 0
Enclosure position: 1
Device Id: 0
WWN: 5002538c4002e713
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SATA

Raw Size: 894.252 GB [0x6fc81ab0 Sectors]
Non Coerced Size: 893.752 GB [0x6fb81ab0 Sectors]
Coerced Size: 893.75 GB [0x6fb80000 Sectors]
Sector Size:  512
Logical Sector Size:  512
Physical Sector Size:  512
Firmware state: Online, Spun Up
Device Firmware Level: 003Q
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x4433221104000000
Connected Port Number: 4(path0)
Inquiry Data: S1YHNXAG804005      SAMSUNG MZ7LM960HCHP-00003              GXT3003Q
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None
Device Speed: 6.0Gb/s
Link Speed: 6.0Gb/s
Media Type: Solid State Device
Drive:  Not Certified
Drive Temperature :33C (91.40 F)
PI Eligibility:  No
Drive is formatted for PI information:  No
PI: No PI
Drive's NCQ setting : N/A
Port-0 :
Port status: Active
Port's Linkspeed: 6.0Gb/s
Drive has flagged a S.M.A.R.T alert : No




PD: 1 Information
Enclosure Device ID: 32
Slot Number: 2
Drive's position: DiskGroup: 0, Span: 0, Arm: 1
Enclosure position: 1
Device Id: 2
WWN: 5002538c00019b96
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SATA

Raw Size: 894.252 GB [0x6fc81ab0 Sectors]
Non Coerced Size: 893.752 GB [0x6fb81ab0 Sectors]
Coerced Size: 893.75 GB [0x6fb80000 Sectors]
Sector Size:  512
Logical Sector Size:  512
Physical Sector Size:  512
Firmware state: Online, Spun Up
Device Firmware Level: 003Q
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x4433221106000000
Connected Port Number: 6(path0)
Inquiry Data: S1YHNYAG600061      SAMSUNG MZ7LM960HCHP-00003              GXT3003Q
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None
Device Speed: 6.0Gb/s
Link Speed: 6.0Gb/s
Media Type: Solid State Device
Drive:  Not Certified
Drive Temperature :33C (91.40 F)
PI Eligibility:  No
Drive is formatted for PI information:  No
PI: No PI
Drive's NCQ setting : N/A
Port-0 :
Port status: Active
Port's Linkspeed: 6.0Gb/s
Drive has flagged a S.M.A.R.T alert : No




PD: 2 Information
Enclosure Device ID: 32
Slot Number: 1
Drive's position: DiskGroup: 0, Span: 0, Arm: 2
Enclosure position: 1
Device Id: 1
WWN: 5002538c4002e707
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SATA

Raw Size: 894.252 GB [0x6fc81ab0 Sectors]
Non Coerced Size: 893.752 GB [0x6fb81ab0 Sectors]
Coerced Size: 893.75 GB [0x6fb80000 Sectors]
Sector Size:  512
Logical Sector Size:  512
Physical Sector Size:  512
Firmware state: Online, Spun Up
Device Firmware Level: 003Q
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x4433221100000000
Connected Port Number: 0(path0)
Inquiry Data: S1YHNXAG803993      SAMSUNG MZ7LM960HCHP-00003              GXT3003Q
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None
Device Speed: 6.0Gb/s
Link Speed: 6.0Gb/s
Media Type: Solid State Device
Drive:  Not Certified
Drive Temperature :34C (93.20 F)
PI Eligibility:  No
Drive is formatted for PI information:  No
PI: No PI
Drive's NCQ setting : N/A
Port-0 :
Port status: Active
Port's Linkspeed: 6.0Gb/s
Drive has flagged a S.M.A.R.T alert : No




PD: 3 Information
Enclosure Device ID: 32
Slot Number: 3
Drive's position: DiskGroup: 0, Span: 0, Arm: 3
Enclosure position: 1
Device Id: 3
WWN: 5002538c4002e70f
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SATA

Raw Size: 894.252 GB [0x6fc81ab0 Sectors]
Non Coerced Size: 893.752 GB [0x6fb81ab0 Sectors]
Coerced Size: 893.75 GB [0x6fb80000 Sectors]
Sector Size:  512
Logical Sector Size:  512
Physical Sector Size:  512
Firmware state: Online, Spun Up
Device Firmware Level: 003Q
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x4433221102000000
Connected Port Number: 2(path0)
Inquiry Data: S1YHNXAG804001      SAMSUNG MZ7LM960HCHP-00003              GXT3003Q
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None
Device Speed: 6.0Gb/s
Link Speed: 6.0Gb/s
Media Type: Solid State Device
Drive:  Not Certified
Drive Temperature :34C (93.20 F)
PI Eligibility:  No
Drive is formatted for PI information:  No
PI: No PI
Drive's NCQ setting : N/A
Port-0 :
Port status: Active
Port's Linkspeed: 6.0Gb/s
Drive has flagged a S.M.A.R.T alert : No




PD: 4 Information
Enclosure Device ID: 32
Slot Number: 5
Drive's position: DiskGroup: 0, Span: 0, Arm: 4
Enclosure position: 1
Device Id: 5
WWN: 5002538c4002e712
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SATA

Raw Size: 894.252 GB [0x6fc81ab0 Sectors]
Non Coerced Size: 893.752 GB [0x6fb81ab0 Sectors]
Coerced Size: 893.75 GB [0x6fb80000 Sectors]
Sector Size:  512
Logical Sector Size:  512
Physical Sector Size:  512
Firmware state: Online, Spun Up
Device Firmware Level: 003Q
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x4433221101000000
Connected Port Number: 1(path0)
Inquiry Data: S1YHNXAG804004      SAMSUNG MZ7LM960HCHP-00003              GXT3003Q
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None
Device Speed: 6.0Gb/s
Link Speed: 6.0Gb/s
Media Type: Solid State Device
Drive:  Not Certified
Drive Temperature :34C (93.20 F)
PI Eligibility:  No
Drive is formatted for PI information:  No
PI: No PI
Drive's NCQ setting : N/A
Port-0 :
Port status: Active
Port's Linkspeed: 6.0Gb/s
Drive has flagged a S.M.A.R.T alert : No




PD: 5 Information
Enclosure Device ID: 32
Slot Number: 4
Drive's position: DiskGroup: 0, Span: 0, Arm: 5
Enclosure position: 1
Device Id: 4
WWN: 5002538c4002e6e9
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SATA

Raw Size: 894.252 GB [0x6fc81ab0 Sectors]
Non Coerced Size: 893.752 GB [0x6fb81ab0 Sectors]
Coerced Size: 893.75 GB [0x6fb80000 Sectors]
Sector Size:  512
Logical Sector Size:  512
Physical Sector Size:  512
Firmware state: Online, Spun Up
Device Firmware Level: 003Q
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x4433221105000000
Connected Port Number: 5(path0)
Inquiry Data: S1YHNXAG803963      SAMSUNG MZ7LM960HCHP-00003              GXT3003Q
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None
Device Speed: 6.0Gb/s
Link Speed: 6.0Gb/s
Media Type: Solid State Device
Drive:  Not Certified
Drive Temperature :33C (91.40 F)
PI Eligibility:  No
Drive is formatted for PI information:  No
PI: No PI
Drive's NCQ setting : N/A
Port-0 :
Port status: Active
Port's Linkspeed: 6.0Gb/s
Drive has flagged a S.M.A.R.T alert : No




PD: 6 Information
Enclosure Device ID: 32
Slot Number: 6
Drive's position: DiskGroup: 0, Span: 0, Arm: 6
Enclosure position: 1
Device Id: 6
WWN: 5002538c4002da83
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SATA

Raw Size: 894.252 GB [0x6fc81ab0 Sectors]
Non Coerced Size: 893.752 GB [0x6fb81ab0 Sectors]
Coerced Size: 893.75 GB [0x6fb80000 Sectors]
Sector Size:  512
Logical Sector Size:  512
Physical Sector Size:  512
Firmware state: Online, Spun Up
Device Firmware Level: 003Q
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x4433221107000000
Connected Port Number: 7(path0)
Inquiry Data: S1YHNXAG801029      SAMSUNG MZ7LM960HCHP-00003              GXT3003Q
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None
Device Speed: 6.0Gb/s
Link Speed: 6.0Gb/s
Media Type: Solid State Device
Drive:  Not Certified
Drive Temperature :33C (91.40 F)
PI Eligibility:  No
Drive is formatted for PI information:  No
PI: No PI
Drive's NCQ setting : N/A
Port-0 :
Port status: Active
Port's Linkspeed: 6.0Gb/s
Drive has flagged a S.M.A.R.T alert : No




PD: 7 Information
Enclosure Device ID: 32
Slot Number: 7
Drive's position: DiskGroup: 0, Span: 0, Arm: 7
Enclosure position: 1
Device Id: 7
WWN: 5002538c4002dade
Sequence Number: 2
Media Error Count: 0
Other Error Count: 0
Predictive Failure Count: 0
Last Predictive Failure Event Seq Number: 0
PD Type: SATA

Raw Size: 894.252 GB [0x6fc81ab0 Sectors]
Non Coerced Size: 893.752 GB [0x6fb81ab0 Sectors]
Coerced Size: 893.75 GB [0x6fb80000 Sectors]
Sector Size:  512
Logical Sector Size:  512
Physical Sector Size:  512
Firmware state: Online, Spun Up
Device Firmware Level: 003Q
Shield Counter: 0
Successful diagnostics completion on :  N/A
SAS Address(0): 0x4433221103000000
Connected Port Number: 3(path0)
Inquiry Data: S1YHNXAG801120      SAMSUNG MZ7LM960HCHP-00003              GXT3003Q
FDE Capable: Not Capable
FDE Enable: Disable
Secured: Unsecured
Locked: Unlocked
Needs EKM Attention: No
Foreign State: None
Device Speed: 6.0Gb/s
Link Speed: 6.0Gb/s
Media Type: Solid State Device
Drive:  Not Certified
Drive Temperature :34C (93.20 F)
PI Eligibility:  No
Drive is formatted for PI information:  No
PI: No PI
Drive's NCQ setting : N/A
Port-0 :
Port status: Active
Port's Linkspeed: 6.0Gb/s
Drive has flagged a S.M.A.R.T alert : No




Exit Code: 0x00