Smart Array P212 in Slot 5
   Bus Interface: PCI
   Slot: 5
   Serial Number: REDACTED
   Cache Serial Number: REDACTED
   Controller Status: OK
   Hardware Revision: C
   Firmware Version: 6.60-0
   Rebuild Priority: Medium
   Expand Priority: Medium
   Surface Scan Delay: 15 secs
   Surface Scan Mode: Idle
   Parallel Surface Scan Supported: No
   Queue Depth: Automatic
   Monitor and Performance Delay: 60  min
   Elevator Sort: Enabled
   Degraded Performance Optimization: Disabled
   Wait for Cache Room: Disabled
   Surface Analysis Inconsistency Notification: Disabled
   Post Prompt Timeout: 0 secs
   Cache Board Present: True
   Cache Status: OK
   Cache Ratio: 100% Read / 0% Write
   Drive Write Cache: Disabled
   Total Cache Size: 0.2
   Total Cache Memory Available: 0.1
   No-Battery Write Cache: Disabled
   SATA NCQ Supported: True
   Number of Ports: 2 (1 Internal / 1 External )
   Encryption: Not Set
   Driver Name: hpsa
   Driver Version: 3.4.20
   Driver Supports SSD Smart Path: True
   PCI Address (Domain:Bus:Device.Function): 0000:14:00.0
   Port Max Phy Rate Limiting Supported: False
   Host Serial Number: REDACTED
   Sanitize Erase Supported: False
   Primary Boot Volume: None
   Secondary Boot Volume: None


   Port Name: 1I
         Port ID: 0
         Port Connection Number: 0
         SAS Address: 5001438014623D00
         Port Location: Internal

   Port Name: 2E
         Port ID: 1
         Port Connection Number: 1
         SAS Address: 5001438014623D04
         Port Location: External


   StorageWorks MSA 60 at Port 2E, Box 1, OK

      Fan Status: OK
      Temperature Status: OK
      Power Supply Status: Redundant
      Vendor ID: HP
      Serial Number:
      Firmware Version: 2.16
      Drive Bays: 12
      Port: 2E
      Box: 1
      Location: External

   Expander 249
      Device Number: 249
      Firmware Version: 2.16
      WWID: REDACTED
      Port: 2E
      Box: 1
      Vendor ID: HP

   Enclosure SEP (Vendor ID HP, Model MSA60) 248
      Device Number: 248
      Firmware Version: 2.16
      WWID: REDACTED
      Port: 2E
      Box: 1
      Vendor ID: HP
      Model: MSA60
      SEP: (1) 2.16
      Backplane Module (BPM): (1) 2.06, (2) 2.06
      Fan Control Module (FCM): (1) 1.08, (2) 1.08
      Health Monitor Module (HMM): (1) 1.10, (2) 1.10
      Seven Segment LED Display: (1) 0.10

   Physical Drives
      physicaldrive 2E:1:1 (port 2E:box 1:bay 1, SATA HDD, 1 TB, OK)
      physicaldrive 2E:1:2 (port 2E:box 1:bay 2, SATA HDD, 1 TB, OK)
      physicaldrive 2E:1:3 (port 2E:box 1:bay 3, SATA HDD, 1 TB, OK)
      physicaldrive 2E:1:4 (port 2E:box 1:bay 4, SATA HDD, 1 TB, OK)
      physicaldrive 2E:1:5 (port 2E:box 1:bay 5, SATA HDD, 1 TB, OK)
      physicaldrive 2E:1:6 (port 2E:box 1:bay 6, SATA HDD, 1 TB, OK)
      physicaldrive 2E:1:7 (port 2E:box 1:bay 7, SATA HDD, 1 TB, OK)
      physicaldrive 2E:1:8 (port 2E:box 1:bay 8, SATA HDD, 1 TB, OK)
      physicaldrive 2E:1:9 (port 2E:box 1:bay 9, SATA HDD, 1 TB, OK)
      physicaldrive 2E:1:10 (port 2E:box 1:bay 10, SATA HDD, 1 TB, OK)
      physicaldrive 2E:1:11 (port 2E:box 1:bay 11, SATA HDD, 1 TB, OK)
      physicaldrive 2E:1:12 (port 2E:box 1:bay 12, SATA HDD, 1 TB, OK)


   Array: A
      Interface Type: SATA
      Unused Space: 0 MB (0.00%)
      Used Space: 5.46 TB (100.00%)
      Status: OK
      Array Type: Data
      Smart Path: disable


      Logical Drive: 1
         Size: 4.55 TB
         Fault Tolerance: 5
         Heads: 255
         Sectors Per Track: 32
         Cylinders: 65535
         Strip Size: 256 KB
         Full Stripe Size: 1280 KB
         Status: OK
         Unrecoverable Media Errors: None
         Caching:  Enabled
         Parity Initialization Status: Initialization Completed
         Unique Identifier: 600508B1001C48AFDD414EB0F3004830
         Disk Name: /dev/sdc
         Mount Points: /srv/mnt2 4.5 TB Partition Number 1
         OS Status: LOCKED
         Logical Drive Label: A4A06DEEPACCPID11170BVJE8DB
         Drive Type: Data
         LD Acceleration Method: Controller Cache


      physicaldrive 2E:1:1
         Port: 2E
         Box: 1
         Bay: 1
         Status: OK
         Drive Type: Data Drive
         Interface Type: SATA
         Size: 1 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 7200
         Firmware Revision: HPG2
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     MB1000EBZQB
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 33
         Maximum Temperature (C): 51
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 2E:1:2
         Port: 2E
         Box: 1
         Bay: 2
         Status: OK
         Drive Type: Data Drive
         Interface Type: SATA
         Size: 1 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 7200
         Firmware Revision: HPG3
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     MB1000EAMZE
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 34
         Maximum Temperature (C): 39
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 2E:1:3
         Port: 2E
         Box: 1
         Bay: 3
         Status: OK
         Drive Type: Data Drive
         Interface Type: SATA
         Size: 1 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 7200
         Firmware Revision: HPG1
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     MB1000ECWCQ
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 35
         Maximum Temperature (C): 41
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 2E:1:4
         Port: 2E
         Box: 1
         Bay: 4
         Status: OK
         Drive Type: Data Drive
         Interface Type: SATA
         Size: 1 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 7200
         Firmware Revision: HPG4
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     MB1000EAMZE
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 35
         Maximum Temperature (C): 44
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 2E:1:5
         Port: 2E
         Box: 1
         Bay: 5
         Status: OK
         Drive Type: Data Drive
         Interface Type: SATA
         Size: 1 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 7200
         Firmware Revision: HPG1
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     MB1000EBZQB
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 34
         Maximum Temperature (C): 51
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 2E:1:6
         Port: 2E
         Box: 1
         Bay: 6
         Status: OK
         Drive Type: Data Drive
         Interface Type: SATA
         Size: 1 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 7200
         Firmware Revision: HPG1
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     MB1000EBZQB
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 33
         Maximum Temperature (C): 50
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None


   Unassigned

      physicaldrive 2E:1:7
         Port: 2E
         Box: 1
         Bay: 7
         Status: OK
         Drive Type: Unassigned Drive
         Interface Type: SATA
         Size: 1 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 7200
         Firmware Revision: HPG2
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     MB1000EBZQB
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 30
         Maximum Temperature (C): 50
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 2E:1:8
         Port: 2E
         Box: 1
         Bay: 8
         Status: OK
         Drive Type: Unassigned Drive
         Interface Type: SATA
         Size: 1 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 7200
         Firmware Revision: HPG1
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     MB1000EAMZE
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 33
         Maximum Temperature (C): 41
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 2E:1:9
         Port: 2E
         Box: 1
         Bay: 9
         Status: OK
         Drive Type: Unassigned Drive
         Interface Type: SATA
         Size: 1 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 7200
         Firmware Revision: HPG1
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     MB1000EBZQB
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 30
         Maximum Temperature (C): 50
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 2E:1:10
         Port: 2E
         Box: 1
         Bay: 10
         Status: OK
         Drive Type: Unassigned Drive
         Interface Type: SATA
         Size: 1 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 7200
         Firmware Revision: HPG2
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     MB1000EBNCF
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 35
         Maximum Temperature (C): 41
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 2E:1:11
         Port: 2E
         Box: 1
         Bay: 11
         Status: OK
         Drive Type: Unassigned Drive
         Interface Type: SATA
         Size: 1 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 7200
         Firmware Revision: HPG1
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     ST31000524NS
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 34
         Maximum Temperature (C): 42
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 2E:1:12
         Port: 2E
         Box: 1
         Bay: 12
         Status: OK
         Drive Type: Unassigned Drive
         Interface Type: SATA
         Size: 1 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 7200
         Firmware Revision: HPG1
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     MB1000EBZQB
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 31
         Maximum Temperature (C): 50
         PHY Count: 1
         PHY Transfer Rate: 1.5Gbps
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None


   Enclosure SEP (Vendor ID HP, Model MSA60) 248
      Device Number: 248
      Firmware Version: 2.16
      WWID: REDACTED
      Port: 2E
      Box: 1
      Vendor ID: HP
      Model: MSA60
      SEP: (1) 2.16
      Backplane Module (BPM): (1) 2.06, (2) 2.06
      Fan Control Module (FCM): (1) 1.08, (2) 1.08
      Health Monitor Module (HMM): (1) 1.10, (2) 1.10
      Seven Segment LED Display: (1) 0.10

   Expander 249
      Device Number: 249
      Firmware Version: 2.16
      WWID: REDACTED
      Port: 2E
      Box: 1
      Vendor ID: HP

   SEP (Vendor ID PMCSIERA, Model  SRC 8x6G) 250
      Device Number: 250
      Firmware Version: RevC
      WWID: REDACTED
      Vendor ID: PMCSIERA
      Model: SRC 8x6G


Smart Array P410i in Slot 0 (Embedded)
   Bus Interface: PCI
   Slot: 0
   Serial Number: REDACTED
   Cache Serial Number: REDACTED
   Controller Status: OK
   Hardware Revision: C
   Firmware Version: 6.40-0
   Rebuild Priority: Medium
   Expand Priority: Medium
   Surface Scan Delay: 15 secs
   Surface Scan Mode: Idle
   Parallel Surface Scan Supported: No
   Queue Depth: Automatic
   Monitor and Performance Delay: 60  min
   Elevator Sort: Enabled
   Degraded Performance Optimization: Disabled
   Wait for Cache Room: Disabled
   Surface Analysis Inconsistency Notification: Disabled
   Post Prompt Timeout: 0 secs
   Cache Board Present: True
   Cache Status: OK
   Cache Ratio: 100% Read / 0% Write
   Drive Write Cache: Disabled
   Total Cache Size: 0.2
   Total Cache Memory Available: 0.1
   No-Battery Write Cache: Disabled
   SATA NCQ Supported: True
   Number of Ports: 2 Internal only
   Encryption: Not Set
   Driver Name: hpsa
   Driver Version: 3.4.20
   Driver Supports SSD Smart Path: True
   PCI Address (Domain:Bus:Device.Function): 0000:04:00.0
   Port Max Phy Rate Limiting Supported: False
   Host Serial Number: REDACTED
   Sanitize Erase Supported: False
   Primary Boot Volume: logicaldrive 1 (600508B1001C8CBE468FB9524F39E535)
   Secondary Boot Volume: None



   Internal Drive Cage at Port 1I, Box 1, OK

      Power Supply Status: Not Redundant
      Drive Bays: 4
      Port: 1I
      Box: 1
      Location: Internal

   Physical Drives
      physicaldrive 1I:1:1 (port 1I:box 1:bay 1, SAS HDD, 146 GB, OK)
      physicaldrive 1I:1:2 (port 1I:box 1:bay 2, SAS HDD, 146 GB, OK)
      physicaldrive 1I:1:3 (port 1I:box 1:bay 3, SAS HDD, 146 GB, OK)
      physicaldrive 1I:1:4 (port 1I:box 1:bay 4, SAS HDD, 146 GB, OK)



   Internal Drive Cage at Port 2I, Box 1, OK

      Power Supply Status: Not Redundant
      Drive Bays: 4
      Port: 2I
      Box: 1
      Location: Internal

   Physical Drives
      physicaldrive 2I:1:5 (port 2I:box 1:bay 5, SAS HDD, 146 GB, OK)
      physicaldrive 2I:1:6 (port 2I:box 1:bay 6, SAS HDD, 146 GB, OK)


   Port Name: 1I
         Port ID: 0
         Port Connection Number: 0
         SAS Address: 50123456789ABCDE
         Port Location: Internal

   Port Name: 2I
         Port ID: 1
         Port Connection Number: 1
         SAS Address: 50123456789ABCE2
         Port Location: Internal

   Array: A
      Interface Type: SAS
      Unused Space: 6 MB (0.00%)
      Used Space: 273.40 GB (100.00%)
      Status: OK
      Array Type: Data
      Smart Path: disable


      Logical Drive: 1
         Size: 136.70 GB
         Fault Tolerance: 1
         Heads: 255
         Sectors Per Track: 32
         Cylinders: 35132
         Strip Size: 256 KB
         Full Stripe Size: 256 KB
         Status: OK
         Unrecoverable Media Errors: None
         Caching:  Enabled
         Unique Identifier: 600508B1001C8CBE468FB9524F39E535
         Disk Name: /dev/sda
         Mount Points: /boot 243 MB Partition Number 1
         OS Status: LOCKED
         Boot Volume: Primary
         Logical Drive Label: ADF758B150123456789ABCDEDC07
         Mirror Group 1:
            physicaldrive 2I:1:5 (port 2I:box 1:bay 5, SAS HDD, 146 GB, OK)
         Mirror Group 2:
            physicaldrive 2I:1:6 (port 2I:box 1:bay 6, SAS HDD, 146 GB, OK)
         Drive Type: Data
         LD Acceleration Method: Controller Cache


      physicaldrive 2I:1:5
         Port: 2I
         Box: 1
         Bay: 5
         Status: OK
         Drive Type: Data Drive
         Interface Type: SAS
         Size: 146 GB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 15000
         Firmware Revision: HPD5 (FW update is recommended to minimum version: HPDA)
         Serial Number: REDACTED
         WWID: REDACTED
         Model: HP      EH0146FARWD
         Current Temperature (C): 38
         Maximum Temperature (C): 38
         PHY Count: 2
         PHY Transfer Rate: 6.0Gbps, Unknown
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 2I:1:6
         Port: 2I
         Box: 1
         Bay: 6
         Status: OK
         Drive Type: Data Drive
         Interface Type: SAS
         Size: 146 GB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 15000
         Firmware Revision: HPDF
         Serial Number: REDACTED
         WWID: REDACTED
         Model: HP      EH0146FAWJB
         Current Temperature (C): 36
         Maximum Temperature (C): 43
         PHY Count: 2
         PHY Transfer Rate: 6.0Gbps, Unknown
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None



   Array: B
      Interface Type: SAS
      Unused Space: 0 MB (0.00%)
      Used Space: 546.81 GB (100.00%)
      Status: OK
      Array Type: Data
      Smart Path: disable


      Logical Drive: 2
         Size: 273.40 GB
         Fault Tolerance: 1+0
         Heads: 255
         Sectors Per Track: 32
         Cylinders: 65535
         Strip Size: 256 KB
         Full Stripe Size: 512 KB
         Status: OK
         Unrecoverable Media Errors: None
         Caching:  Enabled
         Unique Identifier: 600508B1001CE15640A74343E4DD1E18
         Disk Name: /dev/sdb
         Mount Points: /srv/mnt1 262.3 GB Partition Number 1
         OS Status: LOCKED
         Mirror Group 1:
            physicaldrive 1I:1:1 (port 1I:box 1:bay 1, SAS HDD, 146 GB, OK)
            physicaldrive 1I:1:2 (port 1I:box 1:bay 2, SAS HDD, 146 GB, OK)
         Mirror Group 2:
            physicaldrive 1I:1:3 (port 1I:box 1:bay 3, SAS HDD, 146 GB, OK)
            physicaldrive 1I:1:4 (port 1I:box 1:bay 4, SAS HDD, 146 GB, OK)
         Drive Type: Data
         LD Acceleration Method: Controller Cache


      physicaldrive 1I:1:1
         Port: 1I
         Box: 1
         Bay: 1
         Status: OK
         Drive Type: Data Drive
         Interface Type: SAS
         Size: 146 GB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 10000
         Firmware Revision: HPDD
         Serial Number: REDACTED
         WWID: REDACTED
         Model: HP      EG0146FAWHU
         Current Temperature (C): 37
         Maximum Temperature (C): 43
         PHY Count: 2
         PHY Transfer Rate: 6.0Gbps, Unknown
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 1I:1:2
         Port: 1I
         Box: 1
         Bay: 2
         Status: OK
         Drive Type: Data Drive
         Interface Type: SAS
         Size: 146 GB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 10000
         Firmware Revision: HPDD
         Serial Number: REDACTED
         WWID: REDACTED
         Model: HP      EG0146FAWHU
         Current Temperature (C): 37
         Maximum Temperature (C): 44
         PHY Count: 2
         PHY Transfer Rate: 6.0Gbps, Unknown
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 1I:1:3
         Port: 1I
         Box: 1
         Bay: 3
         Status: OK
         Drive Type: Data Drive
         Interface Type: SAS
         Size: 146 GB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 10000
         Firmware Revision: HPDB
         Serial Number: REDACTED
         WWID: REDACTED
         Model: HP      DG146BAAJB
         Current Temperature (C): 43
         Maximum Temperature (C): 52
         PHY Count: 2
         PHY Transfer Rate: 3.0Gbps, Unknown
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 1I:1:4
         Port: 1I
         Box: 1
         Bay: 4
         Status: OK
         Drive Type: Data Drive
         Interface Type: SAS
         Size: 146 GB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/512
         Rotational Speed: 10000
         Firmware Revision: HPDB
         Serial Number: REDACTED
         WWID: REDACTED
         Model: HP      DG146BAAJB
         Current Temperature (C): 44
         Maximum Temperature (C): 55
         PHY Count: 2
         PHY Transfer Rate: 3.0Gbps, Unknown
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None


   SEP (Vendor ID PMCSIERA, Model  SRC 8x6G) 250
      Device Number: 250
      Firmware Version: RevC
      WWID: REDACTED
      Vendor ID: PMCSIERA
      Model: SRC 8x6G
