Smart Array P440ar in Slot 0 (Embedded)
   Bus Interface: PCI
   Slot: 0
   Serial Number: REDACTED
   Cache Serial Number: REDACTED
   RAID 6 (ADG) Status: Enabled
   Controller Status: OK
   Hardware Revision: B
   Firmware Version: 3.56-0
   Rebuild Priority: Low
   Expand Priority: Medium
   Surface Scan Delay: 15 secs
   Surface Scan Mode: Idle
   Parallel Surface Scan Supported: Yes
   Current Parallel Surface Scan Count: 4
   Max Parallel Surface Scan Count: 16
   Queue Depth: Automatic
   Monitor and Performance Delay: 60  min
   Elevator Sort: Enabled
   Degraded Performance Optimization: Disabled
   Inconsistency Repair Policy: Disabled
   Wait for Cache Room: Disabled
   Surface Analysis Inconsistency Notification: Disabled
   Post Prompt Timeout: 0 secs
   Cache Board Present: True
   Cache Status: OK
   Cache Ratio: 10% Read / 90% Write
   Drive Write Cache: Enabled
   Total Cache Size: 2.0 GB
   Total Cache Memory Available: 1.8 GB
   No-Battery Write Cache: Enabled
   SSD Caching RAID5 WriteBack Enabled: True
   SSD Caching Version: 2
   Cache Backup Power Source: Batteries
   Battery/Capacitor Count: 1
   Battery/Capacitor Status: OK
   SATA NCQ Supported: True
   Spare Activation Mode: Activate on physical drive failure (default)
   Controller Temperature (C): 47
   Cache Module Temperature (C): 41
   Number of Ports: 2 Internal only
   Encryption: Disabled
   Express Local Encryption: False
   Driver Name: hpsa
   Driver Version: 3.4.4
   Driver Supports SSD Smart Path: True
   PCI Address (Domain:Bus:Device.Function): 0000:03:00.0
   Negotiated PCIe Data Rate: PCIe 3.0 x8 (7880 MB/s)
   Controller Mode: RAID
   Pending Controller Mode: RAID
   Port Max Phy Rate Limiting Supported: False
   Latency Scheduler Setting: Disabled
   Current Power Mode: MaxPerformance
   Survival Mode: Enabled
   Host Serial Number: REDACTED
   Sanitize Erase Supported: False
   Primary Boot Volume: logicaldrive 1 (600508B1001C158B69C0104DA29E6FF7)
   Secondary Boot Volume: logicaldrive 2 (600508B1001C6BBD22BCA12CEDF36CB0)


   Port Name: 1I
         Port ID: 0
         Port Connection Number: 0
         SAS Address: 5001438037D24990
         Port Location: Internal
         Managed Cable Connected: False

   Port Name: 2I
         Port ID: 1
         Port Connection Number: 1
         SAS Address: 5001438037D24994
         Port Location: Internal
         Managed Cable Connected: False


   Internal Drive Cage at Port 1I, Box 1, OK

      Power Supply Status: Not Redundant
      Drive Bays: 4
      Port: 1I
      Box: 1
      Location: Internal

   Physical Drives
      physicaldrive 1I:1:1 (port 1I:box 1:bay 1, SATA SSD, 1.9 TB, OK)
      physicaldrive 1I:1:2 (port 1I:box 1:bay 2, SATA SSD, 1.9 TB, OK)
      physicaldrive 1I:1:3 (port 1I:box 1:bay 3, SATA SSD, 1.9 TB, OK)
      physicaldrive 1I:1:4 (port 1I:box 1:bay 4, SATA HDD, 1 TB, OK)



   Internal Drive Cage at Port 2I, Box 1, OK

      Power Supply Status: Not Redundant
      Drive Bays: 4
      Port: 2I
      Box: 1
      Location: Internal

   Physical Drives
      physicaldrive 2I:1:5 (port 2I:box 1:bay 5, SATA SSD, 1.9 TB, OK)
      physicaldrive 2I:1:6 (port 2I:box 1:bay 6, SATA SSD, 1.9 TB, OK)
      physicaldrive 2I:1:7 (port 2I:box 1:bay 7, SATA SSD, 1.9 TB, OK)
      physicaldrive 2I:1:8 (port 2I:box 1:bay 8, SATA HDD, 1 TB, OK)


   Array: A
      Interface Type: Solid State SATA
      Unused Space: 0  MB (0.0%)
      Used Space: 10.5 TB (100.0%)
      Status: OK
      MultiDomain Status: OK
      Array Type: Data
      Smart Path: disable


      Logical Drive: 1
         Size: 5.2 TB
         Fault Tolerance: 1+0
         Heads: 255
         Sectors Per Track: 32
         Cylinders: 65535
         Strip Size: 256 KB
         Full Stripe Size: 768 KB
         Status: OK
         MultiDomain Status: OK
         Caching:  Enabled
         Unique Identifier: 600508B1001C158B69C0104DA29E6FF7
         Disk Name: /dev/sda
         Mount Points: / 18.6 GB Partition Number 2, /data 5.2 TB Partition Number 4
         OS Status: LOCKED
         Boot Volume: primary
         Logical Drive Label: A9255E2C50123456789ABCDE7239
         Mirror Group 1:
            physicaldrive 1I:1:1 (port 1I:box 1:bay 1, SATA SSD, 1.9 TB, OK)
            physicaldrive 1I:1:2 (port 1I:box 1:bay 2, SATA SSD, 1.9 TB, OK)
            physicaldrive 1I:1:3 (port 1I:box 1:bay 3, SATA SSD, 1.9 TB, OK)
         Mirror Group 2:
            physicaldrive 2I:1:5 (port 2I:box 1:bay 5, SATA SSD, 1.9 TB, OK)
            physicaldrive 2I:1:6 (port 2I:box 1:bay 6, SATA SSD, 1.9 TB, OK)
            physicaldrive 2I:1:7 (port 2I:box 1:bay 7, SATA SSD, 1.9 TB, OK)
         Drive Type: Data
         LD Acceleration Method: Controller Cache


      physicaldrive 1I:1:1
         Port: 1I
         Box: 1
         Bay: 1
         Status: OK
         Drive Type: Data Drive
         Interface Type: Solid State SATA
         Size: 1.9 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/4096
         Firmware Revision: XCV10110
         Serial Number:REDACTED
         WWID: REDACTED
         Model: ATA     INTEL SSDSC2KB01
         SATA NCQ Capable: True
         SATA NCQ En      physicaldriveabled: True
         Current Temperature (C): 27
         Maximum Temperature (C): 33
         SSD Smart Trip Wearout: Not Supported
         PHY Count: 1
         PHY Transfer Rate: 6.0Gbps
         Drive Authentication Status: OK
         Carrier Application Version: 11
         Carrier Bootloader Version: 6
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 1I:1:2
         Port: 1I
         Box: 1
         Bay: 2
         Status: OK
         Drive Type: Data Drive
         Interface Type: Solid State SATA
         Size: 1.9 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/4096
         Firmware Revision: XCV10110
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     INTEL SSDSC2KB01
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 28
         Maximum Temperature (C): 33
         SSD Smart Trip Wearout: Not Supported
         PHY Count: 1
         PHY Transfer Rate: 6.0Gbps
         Drive Authentication Status: OK
         Carrier Application Version: 11
         Carrier Bootloader Version: 6
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 1I:1:3
         Port: 1I
         Box: 1
         Bay: 3
         Status: OK
         Drive Type: Data Drive
         Interface Type: Solid State SATA
         Size: 1.9 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/4096
         Firmware Revision: XCV10110
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     INTEL SSDSC2KB01
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 27
         Maximum Temperature (C): 30
         SSD Smart Trip Wearout: Not Supported
         PHY Count: 1
         PHY Transfer Rate: 6.0Gbps
         Drive Authentication Status: OK
         Carrier Application Version: 11
         Carrier Bootloader Version: 6
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 2I:1:5
         Port: 2I
         Box: 1
         Bay: 5
         Status: OK
         Drive Type: Data Drive
         Interface Type: Solid State SATA
         Size: 1.9 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/4096
         Firmware Revision: XCV10110
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     INTEL SSDSC2KB01
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 26
         Maximum Temperature (C): 29
         SSD Smart Trip Wearout: Not Supported
         PHY Count: 1
         PHY Transfer Rate: 6.0Gbps
         Drive Authentication Status: OK
         Carrier Application Version: 11
         Carrier Bootloader Version: 6
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 2I:1:6
         Port: 2I
         Box: 1
         Bay: 6
         Status: OK
         Drive Type: Data Drive
         Interface Type: Solid State SATA
         Size: 1.9 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/4096
         Firmware Revision: XCV10110
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     INTEL SSDSC2KB01
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 28
         Maximum Temperature (C): 32
         SSD Smart Trip Wearout: Not Supported
         PHY Count: 1
         PHY Transfer Rate: 6.0Gbps
         Drive Authentication Status: OK
         Carrier Application Version: 11
         Carrier Bootloader Version: 6
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 2I:1:7
         Port: 2I
         Box: 1
         Bay: 7
         Status: OK
         Drive Type: Data Drive
         Interface Type: Solid State SATA
         Size: 1.9 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/4096
         Firmware Revision: XCV10110
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     INTEL SSDSC2KB01
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 27
         Maximum Temperature (C): 32
         SSD Smart Trip Wearout: Not Supported
         PHY Count: 1
         PHY Transfer Rate: 6.0Gbps
         Drive Authentication Status: OK
         Carrier Application Version: 11
         Carrier Bootloader Version: 6
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None



   Array: B
      Interface Type: SATA
      Unused Space: 0  MB (0.0%)
      Used Space: 1.8 TB (100.0%)
      Status: OK
      MultiDomain Status: OK
      Array Type: Data
      Smart Path: disable


      Logical Drive: 2
         Size: 931.5 GB
         Fault Tolerance: 1
         Heads: 255
         Sectors Per Track: 32
         Cylinders: 65535
         Strip Size: 256 KB
         Full Stripe Size: 256 KB
         Status: OK
         MultiDomain Status: OK
         Caching:  Enabled
         Unique Identifier: 600508B1001C6BBD22BCA12CEDF36CB0
         Disk Name: /dev/sdb
         Mount Points: /data/pgsql/spaces/big 931.5 GB Partition Number 1
         OS Status: LOCKED
         Boot Volume: secondary
         Logical Drive Label: A9254E3850123456789ABCDE368D
         Mirror Group 1:
            physicaldrive 1I:1:4 (port 1I:box 1:bay 4, SATA HDD, 1 TB, OK)
         Mirror Group 2:
            physicaldrive 2I:1:8 (port 2I:box 1:bay 8, SATA HDD, 1 TB, OK)
         Drive Type: Data
         LD Acceleration Method: Controller Cache


      physicaldrive 1I:1:4
         Port: 1I
         Box: 1
         Bay: 4
         Status: OK
         Drive Type: Data Drive
         Interface Type: SATA
         Size: 1 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/4096
         Rotational Speed: 5400
         Firmware Revision: 2BA30001
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     ST1000LM024 HN-M
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 30
         Maximum Temperature (C): 35
         PHY Count: 1
         PHY Transfer Rate: 6.0Gbps
         Drive Authentication Status: OK
         Carrier Application Version: 11
         Carrier Bootloader Version: 6
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None

      physicaldrive 2I:1:8
         Port: 2I
         Box: 1
         Bay: 8
         Status: OK
         Drive Type: Data Drive
         Interface Type: SATA
         Size: 1 TB
         Drive exposed to OS: False
         Logical/Physical Block Size: 512/4096
         Rotational Speed: 5400
         Firmware Revision: 2BA30001
         Serial Number: REDACTED
         WWID: REDACTED
         Model: ATA     ST1000LM024 HN-M
         SATA NCQ Capable: True
         SATA NCQ Enabled: True
         Current Temperature (C): 29
         Maximum Temperature (C): 34
         PHY Count: 1
         PHY Transfer Rate: 6.0Gbps
         Drive Authentication Status: OK
         Carrier Application Version: 11
         Carrier Bootloader Version: 6
         Sanitize Erase Supported: False
         Shingled Magnetic Recording Support: None
